





**PATCH PANEL SECTION**



**Place 1 ½” SMRs in PMT clearance holes , either with populated plate minus a few counters, or prior to counter installation for “very close” adjustment.**







**Microscope**

